Title: NOTES:
Author: Rose Bean
Last saved by: rbean
Company: Black & Decker

NOTES:
	1	Date Code located on bottom of housing cover. Remove battery to view.

	8	Torque to 13-18 in.-lbs.

	10	Torque to 22-26 in.-lbs.

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

When servicing Double Insulated Tools, it is extremely important that ONLY IDENTICAL REPLACEMENT PARTS BE USED and that REASSEMBLY OF TOOL IS IDENTICAL TO THE ORIGINAL ASSEMBLY.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.